[image: ]REPV PERMIT PROCESS FLOW CHART

[bookmark: _GoBack]- BUILDING APPLICATION COMPLETED
- ONE SET OF COMPLETE PLANS 
- FIRE DEPARTMENT APPROVAL (if the system has a battery)
(Supporting permit docs if needed like a notarized LOA)
OVER THE COUNTER REVIEW 
(only M & Th 8am-10am or Wed. from 8am-9:30am)
MAX TWO BUILDING PLANS FOR REVIEW PER DAY, PER APPLICANT.  


PHOTOVOLTIC SOLAR SYSTEMS




IF CORRECTIONS:
· RETURN RED MARKED SET
· RESUBMIT A REVISED SET WITH THE INFORMATION DISCLOSED AS REQUESTED
(Ask for resubmittal process handout) 
-DOES THE PROPERTY HAVE 
NON PERMITTED STRUCTURES? (CARPORT, ETC) 
-NON PERMITTED ALTERED STRUCTURES?
(GARAGE CONVERSIONS, ETC)





DURING THE INSPECTION PROCESS

QUALIFIED TECHNICIAN ON SITE

TECHNICIAN SHALL BE FAMILIAR WITH APPROVED PLANS 

COPY OF APPROVED PLANS (PERFORATED PLANS ON SITE)

ROOF ACCESS (LADDER IN PLACE, PROPERLY SECURED, MAY NEED TO BE RELOCATED UPON INSPECTOR REQUEST)

ACCESS TO VERIFY METHODS OF INSTALLATION (OPEN BOXES, PANELS, ETC)

ACCESS TO VERIFY SMOKE DETECTOR AND CARBON MONOXIDE ALARMS 


IF NO: 
[bookmark: _Hlk136327741][bookmark: _Hlk136327742]A BUILDING AND ELECTRICAL PERMIT WILL BE ISSUED AND INSPECTED FOR FINAL APPROVAL 
PROVIDED THE FOLLOWING IS COMPLETED 
YOU MUST SCAN AND UPLOAD THE APPROVED SET OF PLANS ONTO THE PORTAL PIROR TO SCHEDULEING ANY INSPECTION
A BUILDING AND ELECTRICAL PERMIT WILL BE ISSUED AND INSPECTED FOR FINAL APPROVAL 
PROVIDED THE FOLLOWING IS COMPLETED 
(UPLOAD APPROVED SET OF PLANS)
IF YES: 
PLANS WILL CONTAIN LEGIBLE DISCLOSURE AS TO THE AREAS THAT HAVE CODE VIOLATIONS 
(ask for the disclosure notes)
THE CONTRACTOR AGREES TO REMOVE NON PERMITTED ELECTRICAL CONNECTED LOAD TO SYSTEM TO INSPECTOR APPROVAL 
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